{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["【标表2】工程量清单表"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"【标表2】工程量清单表","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"merged":[[1,0,1,6],[2,0,2,4],[4,0,4,6],[26,0,26,2],[28,0,28,2],[29,0,29,6],[30,1,30,6],[31,1,31,6],[32,1,32,6],[33,3,33,4],[33,5,33,6],[34,3,34,4],[34,5,34,6]],"flags":["formulas_cached_only"]}
[]
["工程量清单表"]
["合同段：国道318线黄泥岗至大深村段路面排水及交安工程",{"$nulls":5},"表1"]
[]
["清单"]
["子目号","子目名称","单位","数量","单价","合价","备注"]
["207-1","检查井"]
["-a","雨水检查井混凝土（3000*2000）","m3",130,null,0,"含人工、架管、模板及辅材、井盖安装；混凝土由甲方提供"]
["-b","雨水检查井混凝土","m3",75,null,0,"含人工、模板及辅材、井盖安装；混凝土由甲方提供"]
["-c","雨水检查井钢筋制作、安装","t",10.84,null,0,"含人工、钢筋制作、安装；钢筋由甲方提供"]
["-d","雨水检查井基坑开挖","m3",400,null,0,"含人工基坑开挖、回填、弃方及其运输、辅材，人工挑抬、卷扬机配合"]
["-e","砖砌工程","m3",50,null,0,"含砂浆搅拌、抹面、人工及辅材；砂、水泥由甲方提供"]
["207-3","波纹管"]
["-a","波纹管安装及混凝土浇筑","m",687,null,0,"含人工模板、钢丝网及辅材；混凝土由甲方提供"]
["-b","挖土方","m3",200,null,0,"含人工、管道基坑土方开挖、回填"]
["-c","挖石方","m3",624,null,0,"含人工、管道基坑石方开挖、回填"]
["-d","人工挑抬土方、石方","m3",824,null,0,"含土石弃方，人工挑抬20m高、或卷扬机配合，至弃土场"]
["207-4","支墩"]
["-a","支墩混凝土","m3",112.3,null,0,"含人工、架管、模板及辅材；混凝土由甲方提供"]
["-b","支墩钢筋","t",7.6,null,0,"含人工、钢筋制作、安装；钢筋由甲方提供"]
["-c","人工开挖基坑","m3",200,null,0,"含人工、支墩基坑人工开挖及所需工具、弃方及其运输,人工挑抬、卷扬机配合"]
["207-5","防护栏","m",1250,null,0,"含人工、模板及辅材、钢筋安装、反光标线；混凝土、钢筋由甲方提供"]
["207-6","隔离网","m",1250,null,0,"含人工、安装、安装用螺栓等材料；混凝土、隔离网由甲方提供"]
["207-7","UPVC雨水管安装","m",2000,null,0,"含人工安装；UPVC雨水管由甲方提供"]
[215,"计日工","工日",50,{"v":150,"d":"150.00"},7500]
[]
["投标报价",{"$nulls":4},7500]
["207-2","钢管安装、焊接","m",487,null,0,"此为暂估价，不包含在投标报价，投标人须在施组中对此项工程进行施工说明"]
[]
[]
["填写说明：","1、请各投标人在每一项目中只需填入单价，填入单价后会自动产生投标报价。"]
[null,"2、钢管安装、焊接，作为暂估价，投标人对其计算后作出报价，并在施组中对此项工程进行施工说明，询标时作出阐述。"]
[null,"3、其中计日工单价已固定，投标人不得再进行填报和改动。"]
[{"$nulls":3},"投标人（章）："]
[{"$nulls":3},"日  期：",null,"2018 年 11 月 17 日"]